Note: This API calls are shared between DOS and Win16 personality.

DPMI is a shared interface for DOS applications to access Intel 80286+ CPUs services. DOS DMPI host provides core services for protected mode applications. Multitasking OS with DOS support also provides DMPI in most cases. Windows standard and extended mode kernel is a DPMI client app. Standard and extended mode kernel differs minimally and shares common codebase. Standard Windows kernel works under DOSX extender. DOSX is a specialized version of 16-bit DPMI Extender (but it is standard DPMI host). Standard mode is just DPMI client, exnhanced mode is DPMI client running under Virtual Machime Manager (really, multitasker which allow to run many DOS sessions). Both modes shares DPMI interface for kernel communication. The OS/2 virtual DOS Protected Mode Interface (VDPMI) device driver provides Version 0.9 DPMI support for virtual DOS machines. Win16 (up to Windows ME) provides Version 0.9 DPMI support. Windows in Standard Mode provides DPMI services only for Windows Applications, not DOS sessions.

DPMI host often merged with DPMI extender. Usually DPMI extender provide DPMI host standard services and DOS translation or True DPMI services.

Int 31H, AH=0BH, AL=03H

Version

0.9

Brief

Reset Debug Watchpoint

Input

AX = 0B03H
BX = watchpoint handle

Return

if function successful
Carry flag = clear
if function unsuccessful
Carry flag = set
AX = error code
8023H	invalid handle

Notes

Resets the state of a previously defined debug watchpoint; i.e. a subsequent call to Int 31H Function 0B02H will indicate that the debug watchpoint has not been encountered.

See also

Note

Text based on http://www.delorie.com/djgpp/doc/dpmi/

DPMI
Process manager	INT 2FH 1680H, 1687H
Signals
Memory manager
Misc	INT 2FH 1686H, 168AH
Devices