This is part of Family API which allow to create dual-os version of program runs under OS/2 and DOS

Note: This is legacy API call. It is recommended to use 32-bit equivalent

MouGetNumQueEl

This call returns the current status for the mouse device driver event queue.

Syntax

MouGetNumQueEl (QueDataRecord, DeviceHandle)

Parameters

QueDataRecord (PMOUQUEINFO) - output : Address of the mouse queue status structure:

numqelements (USHORT) : Current number of event queue elements, in the range 0 <> value <> maxnumqelements.

maxnumqelements (USHORT) : Maximum number of queue elements as specified in the QSIZE = NN parameter in DEVICE=MOUSExxx.SYS statement in CONFIG.SYS.

DeviceHandle (HMOU) - input : Contains the handle of the mouse device obtained from a previous MouOpen.

Return Code

rc (USHORT) - return:Return code descriptions are:

0 NO_ERROR

385 ERROR_MOUSE_NO_DEVICE

466 ERROR_MOU_DETACHED

501 ERROR_MOUSE_NO_CONSOLE

505 ERROR_MOU_EXTENDED_SG

Remarks

The maxnumqelements returned by this function is established during mouse device driver configuration. See the mouse DEVICE=MOUSExxx.SYS statement in the IBM Operating System/2 Version 1.2 Command Reference for further details.

Bindings

C

typedef struct _MOUQUEINFO { /* mouqi */ USHORT cEvents; /* current number of event queue elements */ USHORT cmaxEvents; /* MaxNumQueElements value */ } MOUQUEINFO; #define INCL_MOU USHORT rc = MouGetNumQueEl(QueDataRecord, DeviceHandle); PMOUQUEINFO ueDataRecord; /* Ptr to 2-word structure */ HMOU DeviceHandle; /* Mouse device handle */ USHORT rc; /* return code */

MASM

MOUQUEINFO struc mouqi_cEvents dw ? ;current number of event queue elements mouqi_cmaxEvents dw ? ;MaxNumQueElements value MOUQUEINFO ends EXTRN MouGetNumQueEl:FAR INCL_MOU EQU 1 PUSH@ OTHER QueDataRecord ;Ptr to 2-word structure PUSH WORD DeviceHandle ;Mouse device handle CALL MouGetNumQueEl Returns WORD