Note: This IBM PC BIOS API call is for DOS/Win16 personality only. Use Family API for portability.

Note: osFree Macro Library provides macros for most of functions

@Scroll

Brief

Scroll Screen Area Up or Down

Syntax

@Scroll distance, atrib, upcol, uprow, downcol, downrow

BIOS Interrupt

INT10H: H

Family API

fapi

Parameters

distance (BYTE) - rows to scroll

atrib (BYTE) - fill attribute

upcol (BYTE) - upper left column

uprow (BYTE) - upper left row

downcol (BYTE) - down right column

downrow (BYTE) - down right row

Return