FSH_SETVOLUME

Purpose

This function provides the mechanism for assuring that a desired volume is in a removable media drive before I/O is done to the drive.

Calling Sequence

int far pascal FSH_SETVOLUME(hVPB , fControl) unsigned short hVPB; unsigned short fControl;

Where

hVPB is the volume handle for the source of I/O.

fControl is the bit mask of pop-up control actions:

Bit 0 off	indicates volume change pop-up desired
Bit 0 on	indicates no volume change pop-up
All other bits are reserved and must be zero.

Returns

If no error is detected, a zero error code is returned. If an error is detected, one of the following error codes is returned:

ERROR_VOLUME_CHANGED – is an indication that removable media volume change has occurred.

ERROR_INVALID_PARAMETER – the fControl flag word has reserved bits on.

Remarks

This routine is used by the FSH_CALLDRIVER routine to insure that the desired volume is in a removable media drive. FSDs can use it for the same purpose.

FSH_SETVOLUME may block.

Note: OS/2 does not validate input parameters. An FSD, therefore, should call FSH_PROBEBUF where appropriate.