Note: This IBM PC BIOS API call is for DOS/Win16 personality only. Use Family API for portability.

Note: osFree Macro Library provides macros for most of functions

@GetCur

Brief

Get Current Cursor Position and Size

BIOS Interrupt

INT10H: H

Family API

fapi

Syntax

@GetCur page

Parameters

page (BYTE) - optional video page number

Return