Note: This IBM PC BIOS API call is for DOS/Win16 personality only. Use Family API for portability.

Note: osFree Macro Library provides macros for most of functions

@SetCurSz

Brief

Set Cursor Shape Size

BIOS Interrupt

INT10H: H

Family API

fapi

Syntax

INCLUDE BIOS.INC @SetCurSz first, last

Parameters

first (BYTE) - first scan line

last (BYTE) - last scan line

Return

none

Notes

Macro contains bug workaound: AMI 386 BIOS and AST Premier 386 BIOS will lock up the system if AL is not equal to the current video mode