MouFlushQue

Bindings: C, MASM

This call directs the mouse driver to flush (empty) the mouse event queue and the monitor chain data for the session.

MouFlushQue (DeviceHandle)

DeviceHandle (HMOU) - input Mouse device handle from a previous MouOpen.

rc (USHORT) - return Return code descriptions are:

0	NO_ERROR
385	ERROR_MOUSE_NO_DEVICE
466	ERROR_MOU_DETACHED
501	ERROR_MOUSE_NO_CONSOLE
505	ERROR_MOU_EXTENDED_SG