[Q]: Имеется видюшка ATI c 8 мегами. Проблемы с загрузкой оси.

[A]: George Shapovalov (2:5020/341.26)

Hачало Ati.Bug

ATI TECHNOLOGIES INC. CUSTOMER SUPPORT Ref ID: 2573 ATInfo-BASE

The following information applies to IBM OS/2 WARP 4.0

TOPIC: HANGS BOOTING OS/2 WARP 4.0 USING A 3D RAGE II WITH 8MB SGRAM

PRODUCT: 3D PRO TURBO PC2TV 8MB

PROBLEM: System hangs loading OS/2 WARP 4.0 with a 8MB 3D RAGE

PRO TURBO installed.

——————————————————————— SOLUTION: The following procedure will enable you to use the

3D PRO TURBO 8MB card with OS/2 WARP 4.0.

1. Remove the memory module from your 3D PRO TURBO card.
2. Boot to VGA display mode using the following procedure,
During the OS/2 Warp boot process, pressing ALT-F1 when the
block cursor appears in the upper left hand corner will
display a boot menu. Selecting "v" will boot OS/2 WARP in
VGA display mode.
3. Uninstall and re-install the 3.1 OS/2 display drivers.
4. Shutdown OS/2 WARP.
5. Re-install the memory module onto your 3D PRO TURBO card.
6. Restart OS/2 WARP.
! You should be able to access all display modes up to 1280x1024
at 16.7 million colors.

Note: This issue is currently under investigation and will,
hopefully, be resolved with the next release of the
OS/2 display driver.

For more information contact ATI Customer Support and

reference ATInfo-BASE file: 2573

All company and/or product names are trademarks and/or registered trademarks of their respective manufacturers

Конец Ati.Bug